Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 1 : Found directive in column 1. (PROCESSOR)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 3 : Found directive in column 1. (INCLUDE)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\P16F676.INC 41 : Found directive in column 1. (CBLOCK)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\P16F676.INC 66 : Found directive in column 1. (ENDC)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\P16F676.INC 269 : Found directive in column 1. (__CONFIG)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 6 : Found directive in column 1. (ORG)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 13 : Found directive in column 1. (INCLUDE)
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\INTERUPT.ASM 24 : Using default destination of 1 (file).
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 33 : Found directive in column 1. (INCLUDE)
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 58 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 71 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 74 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 77 : Using default destination of 1 (file).
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 86 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 87 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 88 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 89 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 98 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 102 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 104 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 106 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 118 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\ADC.ASM 119 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 34 : Found directive in column 1. (INCLUDE)
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 35 : Found directive in column 1. (INCLUDE)
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 8 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 16 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 19 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Warning[203] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 33 : Found opcode in column 1. (BSF)
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 38 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 50 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 55 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 190 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 199 : Using default destination of 1 (file).
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 207 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 212 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 219 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 224 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 240 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 246 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 251 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 258 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 263 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 278 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 284 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 289 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 296 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\SETUP.ASM 301 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 36 : Found directive in column 1. (INCLUDE)
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\RELE.ASM 66 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\RELE.ASM 106 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\RELE.ASM 117 : Using default destination of 1 (file).
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 37 : Found directive in column 1. (INCLUDE)
Message[302] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 7 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 22 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 23 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 24 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 25 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 26 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 27 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 28 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 57 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 58 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 59 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 80 : Using default destination of 1 (file).
Message[305] D:\PROGRAMS\TEPLOKOM_ST2_SMD\OUT.ASM 96 : Using default destination of 1 (file).
Warning[205] D:\PROGRAMS\TEPLOKOM_ST2_SMD\TEPLOKOM_ST2_SMD.ASM 39 : Found directive in column 1. (END)
