HWiNFO64 v5.72-3333

Creation Time |  | 26.02.2018 20:50 |  |

ASSW-PC

[Current Computer]
| Computer Name: | ASSW-PC
[Operating System]
| Operating System: | Microsoft Windows 7 Ultimate (x64) Build 7601
| Service Pack: | Service Pack 1
| UEFI Boot: | Not Present

Central Processor(s)

[CPU Unit Count]
| Number Of Processor Packages (Physical): | 1
| Number Of Processor Cores: | 4
| Number Of Logical Processors: | 4

AMD Phenom II X4 945

[General Information]
| Processor Name: | AMD Phenom II X4 945
| Original Processor Frequency: | 3000.0 MHz
| Original Processor Frequency [MHz]: | 3000
| CPU ID: | 00100F42
| Extended CPU ID: | 00100F42
| CPU Brand Name: | AMD Phenom(tm) II X4 945 Processor
| CPU Vendor: | AuthenticAMD
| CPU Stepping: | RB-C2 (Ridgeback)
| CPU Code Name: | Deneb
| CPU Technology: | 45 nm
| CPU Thermal Design Power (TDP): | 94.1 W
| CPU Thermal Design Current (TDC): | 72.4 A
| CPU Platform: | Socket AM2r2
| Microcode Update Revision: | 1000086
| Number of CPU Cores: | 4
| Number of Logical CPUs: | 4
[Operating Points]
| CPU HFM (Base): | 3000.0 MHz = 15.00 x 200.0 MHz @ 1.2750 V
| CPU Current: | 3013.7 MHz = 15.00 x 200.9 MHz @ 1.2750 V
| Northbridge Maximum: | 2000.0 MHz = 10.00 x 200.0 MHz @ 1.2750 V
| Northbridge Current: | 1607.3 MHz = 8.00 x 200.9 MHz @ 1.2750 V
| CPU Bus Type: | Hyper-Transport v3.00
| Maximum Supported Hyper-Transport Link Clock: | 2000 MHz
| Current Hyper-Transport Link Clock: | 1004 MHz
[Cache and TLB]
| L1 Cache: | Instruction: 4 x 64 KBytes, Data: 4 x 64 KBytes
| L2 Cache: | Integrated: 4 x 512 KBytes
| L3 Cache: | 6 MBytes
| Instruction TLB: | Fully associative, 32 entries
| Data TLB: | Fully associative, 48 entries
[Standard Feature Flags]
| FPU on Chip | Present
| Enhanced Virtual-86 Mode | Present
| I/O Breakpoints | Present
| Page Size Extensions | Present
| Time Stamp Counter | Present
| Pentium-style Model Specific Registers | Present
| Physical Address Extension | Present
| Machine Check Exception | Present
| CMPXCHG8B Instruction | Present
| APIC On Chip / PGE (AMD) | Present
| Fast System Call | Present
| Memory Type Range Registers | Present
| Page Global Feature | Present
| Machine Check Architecture | Present
| CMOV Instruction | Present
| Page Attribute Table | Present
| 36-bit Page Size Extensions | Present
| Processor Number | Not Present
| CLFLUSH Instruction | Present
| Debug Trace and EMON Store | Not Present
| Internal ACPI Support | Not Present
| MMX Technology | Present
| Fast FP Save/Restore (IA MMX-2) | Present
| Streaming SIMD Extensions | Present
| Streaming SIMD Extensions 2 | Present
| Self-Snoop | Not Present
| Multi-Threading Capable | Present
| Automatic Clock Control | Not Present
| IA-64 Processor | Not Present
| Signal Break on FERR | Not Present
| Streaming SIMD Extensions 3 | Present
| PCLMULQDQ Instruction Support | Not Present
| MONITOR/MWAIT Support | Present
| Supplemental Streaming SIMD Extensions 3 | Not Present
| FMA Extension | Not Present
| CMPXCHG16B Support | Present
| Streaming SIMD Extensions 4.1 | Not Present
| Streaming SIMD Extensions 4.2 | Not Present
| x2APIC | Not Present
| POPCNT Instruction | Present
| AES Cryptography Support | Not Present
| XSAVE/XRSTOR/XSETBV/XGETBV Instructions | Not Present
| XGETBV/XSETBV OS Enabled | Not Present
| AVX Support | Not Present
| Half-Precision Convert (CVT16) | Not Present
[Extended Feature Flags]
| FPU on Chip | Present
| Enhanced Virtual-86 Mode | Present
| I/O Breakpoints | Present
| Page Size Extensions | Present
| Time Stamp Counter | Present
| AMD-style Model Specific Registers | Present
| Machine Check Exception | Present
| CMPXCHG8B Instruction | Present
| APIC On Chip | Present
| SYSCALL and SYSRET Instructions | Present
| Memory Type Range Registers | Present
| Page Global Feature | Present
| Machine Check Architecture | Present
| CMOV Instruction | Present
| Page Attribute Table | Present
| 36-bit Page Size Extensions | Present
| Multi-Processing / Brand feature | Not Present
| No Execute | Present
| MMX Technology | Present
| MMX+ Extensions | Present
| Fast FP Save/Restore | Present
| Fast FP Save/Restore Optimizations | Present
| 1 GB large page support | Present
| RDTSCP Instruction | Present
| x86-64 Long Mode | Present
| 3DNow! Technology Extensions | Present
| 3DNow! Technology | Present
| LAHF/SAHF Long Mode Support | Present
| Core Multi-Processing Legacy Mode | Present
| Secure Virtual Machine | Present
| Extended APIC Register Space | Present
| LOCK MOV CR0 Support | Present
| Advanced Bit Manipulation | Present
| SSE4A Support | Present
| Misaligned SSE Mode | Present
| PREFETCH(W) Support | Present
| OS Visible Work-around Support | Present
| Instruction Based Sampling | Present
| XOP Instruction Support | Not Present
| SKINIT, STGI, and DEV Support | Present
| Watchdog Timer Support | Present
| TBM0 Instruction Support | Not Present
| Lightweight Profiling Support | Not Present
| FMA4 Instruction Support | Not Present
| Translation Cache Extension | Not Present
| NodeId Support | Not Present
| Trailing Bit Manipulation | Not Present
| Topology Extensions | Not Present
| Core Performance Counter Extensions | Not Present
| NB Performance Counter Extensions | Not Present
| Streaming Performance Monitor Architecture | Not Present
| Data Breakpoint Extension | Not Present
| Performance Time-Stamp Counter | Not Present
| L2I Performance Counter Extensions | Not Present
| MWAITX/MONITORX Support | Not Present
| Secure Memory Encryption | Not Present
| Secure Encrypted Virtualization | Not Present
[Enhanced Features]
| Core Performance Boost | Not Supported
[Memory Ranges]
| Maximum Physical Address Size: | 48-bit (256 TBytes)
| Maximum Virtual Address Size: | 48-bit (256 TBytes)
[MTRRs]
| Range 0-80000000 (0MB-2048MB) Type: | Write Back (WB)
| Range 80000000-C0000000 (2048MB-3072MB) Type: | Write Back (WB)

Motherboard

[Computer]
| Computer Brand Name: | Unknown on Noname
[Motherboard]
| Motherboard Model: | ASUS M2N68-AM SE2
| Motherboard Chipset: | nVidia MCP61
| Motherboard Slots: | 1xPCI, 2xPCI Express x1, 1xPCI Express x16
| PCI Express Version Supported: | v1.1
| USB Version Supported: | v2.0
[BIOS]
| BIOS Manufacturer: | American Megatrends
| BIOS Date: | 09/22/09
| BIOS Version: | 1002
| AMD AGESA Version: | 2.3.3
| UEFI BIOS: | Not Capable
| Super-IO/LPC Chip: | ITE IT8712F, Rev J/K

ACPI Devices

Процессор AMD

| Device Name: | Процессор AMD

Процессор AMD

| Device Name: | Процессор AMD

Процессор AMD

| Device Name: | Процессор AMD

Процессор AMD

| Device Name: | Процессор AMD

Фиксированная функциональная кнопка ACPI

| Device Name: | Фиксированная функциональная кнопка ACPI

Программируемый контроллер прерываний

| Device Name: | Программируемый контроллер прерываний
[Assigned Resources]
| I/O Port: | 0020 - 0021
| IRQ: | 65792
[Alternative 1]
| I/O Port: | 0020 - 0021
| I/O Port: | 00A0 - 00A1

Системный таймер

| Device Name: | Системный таймер
[Assigned Resources]
| I/O Port: | 0040 - 0043
[Alternative 1]
| I/O Port: | 0040 - 0043
| IRQ: | 0

Высокоточный таймер событий

| Device Name: | Высокоточный таймер событий
[Assigned Resources]
| Memory Location: | FED00000 - FED00FFF
[Alternative 1]
| Memory Location: | FED00000 - FED00FFF

Контроллер прямого доступа к памяти

| Device Name: | Контроллер прямого доступа к памяти
[Assigned Resources]
| I/O Port: | 0089 - 008B
| DMA: | 4
[Alternative 1]
| I/O Port: | 0000 - 000F
| I/O Port: | 0081 - 0083
| I/O Port: | 0087
| I/O Port: | 0089 - 008B
| I/O Port: | 008F
| I/O Port: | 00C0 - 00DF
| DMA: | 4

Стандартная клавиатура PS/2

| Device Name: | Стандартная клавиатура PS/2
[Assigned Resources]
| I/O Port: | 0060
| I/O Port: | 0000
[Alternative 1]
| I/O Port: | 0060
| I/O Port: | 0064
| IRQ: | 1

Последовательный порт

| Device Name: | Последовательный порт
[Assigned Resources]
| I/O Port: | 03F8 - 03FF
[Alternative 1]
| I/O Port: | 03F8 - 03FF
| IRQ: | 4
[Alternative 2]
| I/O Port: | 03F8 - 03FF
| IRQ: | 3
| IRQ: | 4
| IRQ: | 5
| IRQ: | 6
| IRQ: | 7
| IRQ: | 10
| IRQ: | 11
| IRQ: | 12
[Alternative 3]
| I/O Port: | 02F8 - 02FF
| IRQ: | 3
| IRQ: | 4
| IRQ: | 5
| IRQ: | 6
| IRQ: | 7
| IRQ: | 10
| IRQ: | 11
| IRQ: | 12
[Alternative 4]
| I/O Port: | 03E8 - 03EF
| IRQ: | 3
| IRQ: | 4
| IRQ: | 5
| IRQ: | 6
| IRQ: | 7
| IRQ: | 10
| IRQ: | 11
| IRQ: | 12
[Alternative 5]
| I/O Port: | 02E8 - 02EF
| IRQ: | 3
| IRQ: | 4
| IRQ: | 5
| IRQ: | 6
| IRQ: | 7
| IRQ: | 10
| IRQ: | 11
| IRQ: | 12

Встроенный динамик

| Device Name: | Встроенный динамик
[Assigned Resources]
| I/O Port: | 0061
[Alternative 1]
| I/O Port: | 0061

Шина PCI

| Device Name: | Шина PCI
[Assigned Resources]
| I/O Port: | 0000 - FFFFFFFF
| Memory Location: | 000A0000 - 000BFFFF
| Memory Location: | C0000000 - BFFFFFFF
[Alternative 1]
| I/O Port: | 0000 - 0CF7
| I/O Port: | 0D00 - FFFF
| Memory Location: | 000A0000 - 000BFFFF
| Memory Location: | 000D0000 - 000DFFFF
| Memory Location: | C0000000 - DFFFFFFF
| Memory Location: | F0000000 - FEBFFFFF

CMOS и часы

| Device Name: | CMOS и часы
[Assigned Resources]
| I/O Port: | 0070 - 0071
[Alternative 1]
| I/O Port: | 0070 - 0071
| IRQ: | 8

Системная плата

| Device Name: | Системная плата
[Assigned Resources]
| Memory Location: | 00000000 - 0009FFFF
[Alternative 1]
| Memory Location: | 00000000 - 0009FFFF
| Memory Location: | 000C0000 - 000CFFFF
| Memory Location: | 000E0000 - 000FFFFF
| Memory Location: | 00100000 - BFFFFFFF
| Memory Location: | FEC00000 - FFFFFFFF

Ресурсы системной платы

| Device Name: | Ресурсы системной платы
[Assigned Resources]
| Memory Location: | FEC00000 - FEC00FFF
[Alternative 1]
| Memory Location: | FEC00000 - FEC00FFF
| Memory Location: | FEE00000 - FEE00FFF

Ресурсы системной платы

| Device Name: | Ресурсы системной платы
[Assigned Resources]
| I/O Port: | 0050 - 005F
| I/O Port: | 0080
| I/O Port: | 0090 - 009F
| I/O Port: | 0800 - 080F
| I/O Port: | 0880 - 08FF
| Memory Location: | 000D0000 - 000D3FFF
| Memory Location: | 000DE000 - 000DDFFF
| Memory Location: | 00000000 - 00000087
| IRQ: | 1114369
[Alternative 1]
| I/O Port: | 0010 - 001F
| I/O Port: | 0022 - 003F
| I/O Port: | 0044 - 004D
| I/O Port: | 0050 - 005F
| I/O Port: | 0062 - 0063
| I/O Port: | 0065 - 006F
| I/O Port: | 0072 - 007F
| I/O Port: | 0080
| I/O Port: | 0084 - 0086
| I/O Port: | 0088
| I/O Port: | 008C - 008E
| I/O Port: | 0090 - 009F
| I/O Port: | 00A2 - 00BF
| I/O Port: | 00E0 - 00EF
| I/O Port: | 04D0 - 04D1
| I/O Port: | 0800 - 080F
| I/O Port: | 0500 - 057F
| I/O Port: | 0580 - 05FF
| I/O Port: | 0800 - 087F
| I/O Port: | 0880 - 08FF
| I/O Port: | 0D00 - 0D7F
| I/O Port: | 0D80 - 0DFF
| I/O Port: | 0900 - 097F
| I/O Port: | 0980 - 09FF
| I/O Port: | 1100 - 117F
| I/O Port: | 1180 - 11FF
| Memory Location: | 000D0000 - 000D3FFF
| Memory Location: | 000D4000 - 000D7FFF
| Memory Location: | 000DE000 - 000DFFFF
| Memory Location: | FEC80000 - FD93FFFF
| Memory Location: | FEFE0000 - FEFE01FF
| Memory Location: | FEFE1000 - FEFE1FFF
| Memory Location: | FEE01000 - FEEFFFFF

Ресурсы системной платы

| Device Name: | Ресурсы системной платы
[Assigned Resources]
| Memory Location: | E0000000 - EFFFFFFF
[Alternative 1]
| Memory Location: | E0000000 - EFFFFFFF

Ресурсы системной платы

| Device Name: | Ресурсы системной платы
[Assigned Resources]
| I/O Port: | 0230 - 023F
[Alternative 1]
| I/O Port: | 0230 - 023F
| I/O Port: | 0290 - 029F
| I/O Port: | 0A00 - 0A0F
| I/O Port: | 0A10 - 0A1F

Арифметический сопроцессор

| Device Name: | Арифметический сопроцессор
[Assigned Resources]
| I/O Port: | 00F0 - 00FF
[Alternative 1]
| I/O Port: | 00F0 - 00FF
| IRQ: | 13

Кнопка питания ACPI

| Device Name: | Кнопка питания ACPI

SMBIOS DMI

BIOS

| BIOS Vendor: | American Megatrends Inc.
| BIOS Version: | 1002
| BIOS Release Date: | 09/22/2009
| BIOS Start Segment: | F000
| BIOS Size: | 1024 KBytes
| System BIOS Version: | 8.14
| ISA Support: | Present
| MCA Support: | Not Present
| EISA Support: | Not Present
| PCI Support: | Present
| PC Card (PCMCIA) Support: | Not Present
| Plug-and-Play Support: | Present
| APM Support: | Present
| Flash BIOS: | Present
| BIOS Shadow: | Present
| VL-VESA Support: | Not Present
| ESCD Support: | Present
| Boot from CD: | Present
| Selectable Boot: | Present
| BIOS ROM Socketed: | Present
| Boot from PC Card: | Not Present
| EDD Support: | Present
| NEC PC-98 Support: | Not Present
| ACPI Support: | Present
| USB Legacy Support: | Present
| AGP Support: | Not Present
| I2O Boot Support: | Not Present
| LS-120 Boot Support: | Present
| ATAPI ZIP Drive Boot Support: | Present
| IEE1394 Boot Support: | Not Present
| Smart Battery Support: | Not Present
| BIOS Boot Specification Support: | Present
| Function key-initiated Network Service Boot Support: | Not Present
| Targeted Content Distribution Support: | Present
| UEFI Specification Support: | Not Present
| Virtual Machine: | Not Present

System

| System Manufacturer: | System manufacturer
| Product Name: | System Product Name
| Product Version: | System Version
| Product Serial Number: | System Serial Number
| UUID: | {EE1F7C80-FE8D-11D5-90F7-002618E6E7AF}
| SKU Number: | To Be Filled By O.E.M.
| Family: | To Be Filled By O.E.M.

Mainboard

| Mainboard Manufacturer: | ASUSTeK Computer INC.
| Mainboard Name: | M2N68-AM SE2
| Mainboard Version: | Rev X.0x
| Mainboard Serial Number: | MF7099G07101040
| Asset Tag: | To Be Filled By O.E.M.
| Location in chassis: | To Be Filled By O.E.M.

System Enclosure

| Manufacturer: | Chassis Manufacture
| Case Type: | Desktop
| Version: | Chassis Version
| Serial Number: | Chassis Serial Number
| Asset Tag Number: | Asset-1234567890

Processor

| Processor Manufacturer: | AMD
| Processor Version: | AMD Phenom(tm) II X4 945 Processor
| External Clock: | 200 MHz
| Maximum Clock Supported: | 3000 MHz
| Current Clock: | 3000 MHz
| CPU Socket: | Populated
| CPU Status: | Enabled
| Processor Type: | Central Processor
| Processor Voltage: | 1.5 V
| Processor Upgrade: | Unknown (1)
| Socket Designation: | AM2

L1-Cache

| Socket Designation: | L1-Cache
| Cache State: | Enabled
| Cache Type: | Internal, Data
| Cache Scheme: | Write-Through and Write-Back
| Supported SRAM Type: | Pipeline Burst
| Current SRAM Type: | Pipeline Burst
| Cache Speed: | Unknown
| Error Correction Type: | Single-bit ECC
| Maximum Cache Size: | 512 KBytes
| Installed Cache Size: | 512 KBytes
| Cache Associativity: | 4-way Set-Associative

L2-Cache

| Socket Designation: | L2-Cache
| Cache State: | Enabled
| Cache Type: | Internal, Unified
| Cache Scheme: | Write-Through and Write-Back
| Supported SRAM Type: | Pipeline Burst
| Current SRAM Type: | Pipeline Burst
| Cache Speed: | Unknown
| Error Correction Type: | Single-bit ECC
| Maximum Cache Size: | 2048 KBytes
| Installed Cache Size: | 2048 KBytes
| Cache Associativity: | 4-way Set-Associative

L3-Cache

| Socket Designation: | L3-Cache
| Cache State: | Enabled
| Cache Type: | Internal, Unified
| Cache Scheme: | Write-Through and Write-Back
| Supported SRAM Type: | Pipeline Burst
| Current SRAM Type: | Pipeline Burst
| Cache Speed: | Unknown
| Error Correction Type: | Single-bit ECC
| Maximum Cache Size: | 6144 KBytes
| Installed Cache Size: | 6144 KBytes
| Cache Associativity: | 4-way Set-Associative

On Board Device

| Device Description: | To Be Filled By O.E.M.
| Device Type: | Video Adapter
| Device Status: | Enabled

OEM Strings

|  | 002618E6E7AF
|  | To Be Filled By O.E.M.
|  | To Be Filled By O.E.M.
|  | To Be Filled By O.E.M.

BIOS Language

|  | en|US|iso8859-1 <Active>

System Boot Information

| Boot Status: | No error occured

Memory Devices

Memory Controller

| Error Detecting Method: | 64-bit ECC
| Error Correction: | None
| Supported Interleave: | 1-Way
| Current Interleave: | 1-Way
| Max. Memory Module Size: | 2048 MBytes
| Supported Memory Speed: | 70 ns, 60 ns
| Supported Memory Type: | DIMM, SDRAM
| Supported Memory Voltage: | 3.3 V
| Associated Memory Slots: | 2

DIMM0

| Socket Designation: | DIMM0
| Memory Type: | DIMM
| Memory Speed: | 25 ns
| Installed size: | 2048 MBytes
| Enabled size: | 2048 MBytes

DIMM1

| Socket Designation: | DIMM1
| Memory Type: | DIMM
| Memory Speed: | 25 ns
| Installed size: | 2048 MBytes
| Enabled size: | 2048 MBytes

Physical Memory Array

| Array Location: | System board
| Array Use: | System memory
| Error Detecting Method: | None
| Memory Capacity: | 4 GBytes
| Memory Devices: | 2

Memory Array Mapped Address

| Starting Address: | 00000000
| Ending Address: | 004FFFFF
| Partition Width: | 1

Memory Device

| Total Width: | 64 bits
| Data Width: | 64 bits
| Device Size: | 2048 MBytes
| Device Form Factor: | DIMM
| Device Locator: | DIMM0
| Bank Locator: | BANK0
| Device Type: | DDR2 SDRAM
| Device Type Detail: | Synchronous
| Memory Speed: | 800 MHz
| Manufacturer: | Manufacturer0
| Serial Number: | SerNum0
| Part Number: | PartNum0
| Asset Tag: | AssetTagNum0

Memory Device Mapped Address

| Starting Address: | 00000000
| Ending Address: | 001FFFFF
| Partition Row Position: | 1
| Interleave Position: | Non-interleaved
| Interleave Data Depth: | 0

Memory Device

| Total Width: | 64 bits
| Data Width: | 64 bits
| Device Size: | 2048 MBytes
| Device Form Factor: | DIMM
| Device Locator: | DIMM1
| Bank Locator: | BANK1
| Device Type: | DDR2 SDRAM
| Device Type Detail: | Synchronous
| Memory Speed: | 800 MHz
| Manufacturer: | Manufacturer1
| Serial Number: | SerNum1
| Part Number: | PartNum1
| Asset Tag: | AssetTagNum1

Memory Device Mapped Address

| Starting Address: | 00200000
| Ending Address: | 003FFFFF
| Partition Row Position: | 1
| Interleave Position: | Non-interleaved
| Interleave Data Depth: | 0

Port Connectors

Mouse Port

| Port Type: | Mouse Port
| Internal Reference: | KBMS
| Internal Connector Type: | None
| External Reference: | KBMS
| External Connector Type: | PS/2

USB

| Port Type: | USB
| Internal Reference: | USB12
| Internal Connector Type: | None
| External Reference: | USB12
| External Connector Type: | Access Bus (USB)

USB

| Port Type: | USB
| Internal Reference: | USB34
| Internal Connector Type: | None
| External Reference: | USB34
| External Connector Type: | Access Bus (USB)

USB

| Port Type: | USB
| Internal Reference: | USB56
| Internal Connector Type: | None
| External Reference: | USB56
| External Connector Type: | Access Bus (USB)

USB

| Port Type: | USB
| Internal Reference: | USB78
| Internal Connector Type: | None
| External Reference: | USB78
| External Connector Type: | Access Bus (USB)

USB

| Port Type: | USB
| Internal Reference: | USB910
| Internal Connector Type: | None
| External Reference: | USB910
| External Connector Type: | Access Bus (USB)

Serial Port 16550A Compatible

| Port Type: | Serial Port 16550A Compatible
| Internal Reference: | COM Port
| Internal Connector Type: | None
| External Reference: | COM A
| External Connector Type: | DB-9 pin male

Audio Port

| Port Type: | Audio Port
| Internal Reference: | Audio_Line_In
| Internal Connector Type: | None
| External Reference: | Audio_Line_In
| External Connector Type: | Mini-jack (headphones)

Audio Port

| Port Type: | Audio Port
| Internal Reference: | Audio_Line_Out
| Internal Connector Type: | None
| External Reference: | Audio_Line_Out
| External Connector Type: | Mini-jack (headphones)

Audio Port

| Port Type: | Audio Port
| Internal Reference: | Audio_Mic_In
| Internal Connector Type: | None
| External Reference: | Audio_Mic_In
| External Connector Type: | Mini-jack (headphones)

Network Port

| Port Type: | Network Port
| Internal Reference: | LAN
| Internal Connector Type: | None
| External Reference: | LAN
| External Connector Type: | RJ-45

Port Connector

| Port Type: | Unknown
| Internal Reference: | D-Sub
| Internal Connector Type: | None
| External Reference: | D-Sub port
| External Connector Type: | Unknown

Port Connector

| Port Type: | Unknown
| Internal Reference: | CD
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | PRI IDE
| Internal Connector Type: | On Board IDE
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | AAFP
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | PANEL
| Internal Connector Type: | 9 Pin Dual Inline (pin 10 cut)
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | SPEAKER
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | CPU FAN
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | CHA FAN
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | SATA1
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

Port Connector

| Port Type: | Unknown
| Internal Reference: | SATA2
| Internal Connector Type: | Unknown
| External Reference: | Unknown
| External Connector Type: | None

System Slots

PCIEX16

| Slot Designation: | PCIEX16
| Slot Type: | PCI Express
| Slot Usage: | In use
| Slot Data Bus Width: | 16x / x16
| Slot Length: | Short

PCIEX1

| Slot Designation: | PCIEX1
| Slot Type: | PCI Express
| Slot Usage: | Empty
| Slot Data Bus Width: | 1x / x1
| Slot Length: | Short

PCI1

| Slot Designation: | PCI1
| Slot Type: | PCI
| Slot Usage: | Empty
| Slot Data Bus Width: | 32-bit
| Slot Length: | Short

Memory

[General information]
| Total Memory Size: | 4 GBytes
| Total Memory Size [MB]: | 4096
[Current Performance Settings]
| Maximum Supported Memory Clock: | 666.7 MHz
| Current Memory Clock: | 401.8 MHz (2 : 1 ratio)
| Current Timing (tCAS-tRCD-tRP-tRAS): | 5-5-5-18
| Memory Runs At: | Dual-Channel
| Command Rate: | 2T
| Read to Read Delay (tRD_RD) Different Rank: | 3T
| Write to Write Delay (tWR_WR) Different Rank: | 1T
| Write to Read Delay (tWR_RD) Same Rank (tWTR): | 3T
| Write to Precharge Delay (tWTP): | 17T
| Write Recovery Time (tWR): | 6T
| RAS# to RAS# Delay (tRRD): | 3T
| Row Cycle Time (tRC): | 23T
| Four Activate Window (tFAW): | 14T

Row: 0 - 2 GB PC2-6400 DDR2-SDRAM Kingmax Semiconductor KLDE88F-B8KU5

[General Module Information]
| Module Number: | 0
| Module Size: | 2 GBytes
| Memory Type: | DDR2-SDRAM
| Module Type: | Regular Unbuffered (UDIMM)
| Error Check/Correction: | None
| Memory Speed: | 400.0 MHz (PC2-6400)
| Module Manufacturer: | Kingmax Semiconductor
| Module Part Number: | KLDE88F-B8KU5
| Module Serial Number: | N/A
| Module Manufacturing Date: | Unknown
[Module Characteristics]
| Module Width: | 64-bits
| Module Voltage: | SSTL 1.8V
| SPD Revision: | 1.2
| Number Of Ranks: | 2
| Row Address Bits: | 14
| Column Address Bits: | 10
| Number Of Banks: | 8
[Module timing]
| Supported Burst Lengths: | 4, 8
| Refresh Rate: | Reduced 0.5x (7.8 us)
| Supported CAS Latencies (tCAS): | 5.0, 4.0, 3.0
| Min. RAS-to-CAS Delay (tRCD): | 12.50 ns
| Min. Row Precharge Time (tRP): | 12.50 ns
| Min. RAS Pulse Width (tRAS): | 45 ns
| Supported Module Timing at 400.0 MHz: | 5.0-5-5-18
| Supported Module Timing at 266.7 MHz: | 4.0-4-4-12
| Supported Module Timing at 200.0 MHz: | 3.0-3-3-9
| Min. Row-Activate To Row-Activate Delay (tRRD): | 7.50 ns
| Write Recovery Time (tWR): | 15.00 ns
| Internal write to read command delay (tWTR): | 7.50 ns
| Internal read to precharge command delay (tRTP): | 7.50 ns
| Minimum Activate to Activate/Refresh Time (tRC): | 57.00 ns
| Minimum Refresh to Activate/Refresh Command Period (tRFC): | 127.00 ns
| Address and Command Setup Time Before Clock (tIS): | 0.17 ns
| Address and Command Setup Time After Clock (tIH): | 0.25 ns
| Data Input Setup Time Before Strobe (tDS): | 0.05 ns
| Data Input Setup Time After Strobe (tDH): | 0.12 ns

Row: 1 - 2 GB PC2-6400 DDR2-SDRAM Kingmax Semiconductor KLDE88F-B8KU5

[General Module Information]
| Module Number: | 1
| Module Size: | 2 GBytes
| Memory Type: | DDR2-SDRAM
| Module Type: | Regular Unbuffered (UDIMM)
| Error Check/Correction: | None
| Memory Speed: | 400.0 MHz (PC2-6400)
| Module Manufacturer: | Kingmax Semiconductor
| Module Part Number: | KLDE88F-B8KU5
| Module Serial Number: | N/A
| Module Manufacturing Date: | Unknown
[Module Characteristics]
| Module Width: | 64-bits
| Module Voltage: | SSTL 1.8V
| SPD Revision: | 1.2
| Number Of Ranks: | 2
| Row Address Bits: | 14
| Column Address Bits: | 10
| Number Of Banks: | 8
[Module timing]
| Supported Burst Lengths: | 4, 8
| Refresh Rate: | Reduced 0.5x (7.8 us)
| Supported CAS Latencies (tCAS): | 5.0, 4.0, 3.0
| Min. RAS-to-CAS Delay (tRCD): | 12.50 ns
| Min. Row Precharge Time (tRP): | 12.50 ns
| Min. RAS Pulse Width (tRAS): | 45 ns
| Supported Module Timing at 400.0 MHz: | 5.0-5-5-18
| Supported Module Timing at 266.7 MHz: | 4.0-4-4-12
| Supported Module Timing at 200.0 MHz: | 3.0-3-3-9
| Min. Row-Activate To Row-Activate Delay (tRRD): | 7.50 ns
| Write Recovery Time (tWR): | 15.00 ns
| Internal write to read command delay (tWTR): | 7.50 ns
| Internal read to precharge command delay (tRTP): | 7.50 ns
| Minimum Activate to Activate/Refresh Time (tRC): | 57.00 ns
| Minimum Refresh to Activate/Refresh Command Period (tRFC): | 127.00 ns
| Address and Command Setup Time Before Clock (tIS): | 0.17 ns
| Address and Command Setup Time After Clock (tIH): | 0.25 ns
| Data Input Setup Time Before Strobe (tDS): | 0.05 ns
| Data Input Setup Time After Strobe (tDH): | 0.12 ns

Bus

PCI Bus #0

NVIDIA MCP61 - LPC Bridge

[General Information]
| Device Name: | NVIDIA MCP61 - LPC Bridge
| Original Device Name: | NVIDIA MCP61 - LPC Bridge
| Device Class: | RAM/Memory Controller
| Revision ID: | A1
| PCI Address (Bus:Device:Function) Number: | 0:0:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03E2&SUBSYS_83A41043&REV_A1
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный PCI-контроллер RAM
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03E2&SUBSYS_83A41043&REV_A1\3&267A616A&0&00
| Location Paths | PCIROOT(0)#PCI(0000)

NVIDIA MCP61 - LPC Bridge

[General Information]
| Device Name: | NVIDIA MCP61 - LPC Bridge
| Original Device Name: | NVIDIA MCP61 - LPC Bridge
| Device Class: | PCI-to-ISA Bridge
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:1:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03E1&SUBSYS_83A41043&REV_A2
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
| I/O Base Address 0 | 900
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - ISA
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03E1&SUBSYS_83A41043&REV_A2\3&267A616A&0&08
| Location Paths | PCIROOT(0)#PCI(0100)

NVIDIA MCP61 - SMBus Controller

[General Information]
| Device Name: | NVIDIA MCP61 - SMBus Controller
| Original Device Name: | NVIDIA MCP61 - SMBus Controller
| Device Class: | SMBus (System Management Bus)
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:1:1
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03EB&SUBSYS_83A41043&REV_A2
[System Resources]
| Interrupt Line: | IRQ10
| Interrupt Pin: | INTA#
| I/O Base Address 0 | E00
| I/O Base Address 4 | 600
| I/O Base Address 5 | 700
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | NVIDIA
| Driver Description: | NVIDIA nForce PCI System Management
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03EB&SUBSYS_83A41043&REV_A2\3&267A616A&0&09
| Location Paths | PCIROOT(0)#PCI(0101)

NVIDIA MCP61 - Memory Controller

[General Information]
| Device Name: | NVIDIA MCP61 - Memory Controller
| Original Device Name: | NVIDIA MCP61 - Memory Controller
| Device Class: | RAM/Memory Controller
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:1:2
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03F5&SUBSYS_83A41043&REV_A2
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный PCI-контроллер RAM
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03F5&SUBSYS_83A41043&REV_A2\3&267A616A&0&0A
| Location Paths | PCIROOT(0)#PCI(0102)

NVIDIA MCP61 - OHCI USB 1.1 Controller

[General Information]
| Device Name: | NVIDIA MCP61 - OHCI USB 1.1 Controller
| Original Device Name: | NVIDIA MCP61 - OHCI USB 1.1 Controller
| Device Class: | USB OHCI Controller
| Revision ID: | A3
| PCI Address (Bus:Device:Function) Number: | 0:2:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03F1&SUBSYS_83A41043&REV_A3
[System Resources]
| Interrupt Line: | IRQ22
| Interrupt Pin: | INTA#
| Memory Base Address 0 | DFEFF000
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
| USB Version Supported: | 1.0
[Driver Information]
| Driver Manufacturer: | (Стандартный USB хост-контроллер)
| Driver Description: | Стандартный OpenHCD USB хост-контроллер
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.23933
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03F1&SUBSYS_83A41043&REV_A3\3&267A616A&0&10
| Location Paths | PCIROOT(0)#PCI(0200)

USB Root Hub

[Port1] : No Device Connected

[Port2] : No Device Connected

[Port3] : Составное USB устройство

[Device Information]
| Device Manufacturer: | A4TECH
| Product Name: | USB Device
| Serial Number: | N/A
| USB Version Supported: | 1.10
| USB Device Speed: | USB 1.1 Full-speed
| Driver Description: | Составное USB устройство
| Hardware ID: | USB\VID_09DA&PID_9090
[Driver Information]
| Driver Manufacturer: | (Стандартный USB хост-контроллер)
| Driver Description: | Составное USB устройство
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.23933
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | USB\VID_09DA&PID_9090\5&13FF92DD&0&3
| Location Paths | PCIROOT(0)#PCI(0200)#USBROOT(0)#USB(3)

[Port4] : No Device Connected

[Port5] : No Device Connected

[Port6] : No Device Connected

[Port7] : No Device Connected

[Port8] : No Device Connected

[Port9] : No Device Connected

[Port10] : No Device Connected

NVIDIA MCP61 - EHCI USB 2.0 Controller

[General Information]
| Device Name: | NVIDIA MCP61 - EHCI USB 2.0 Controller
| Original Device Name: | NVIDIA MCP61 - EHCI USB 2.0 Controller
| Device Class: | USB EHCI Controller
| Revision ID: | A3
| PCI Address (Bus:Device:Function) Number: | 0:2:1
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03F2&SUBSYS_83A41043&REV_A3
[System Resources]
| Interrupt Line: | IRQ21
| Interrupt Pin: | INTB#
| Memory Base Address 0 | DFEFEC00
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
| USB Version Supported: | 2.0
[Driver Information]
| Driver Manufacturer: | (Стандартный USB хост-контроллер)
| Driver Description: | Стандартный расширенный PCI - USB хост-контроллер
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.23933
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03F2&SUBSYS_83A41043&REV_A3\3&267A616A&0&11
| Location Paths | PCIROOT(0)#PCI(0201)

USB Root Hub

[Port1] : Logitech USB Camera (HD Webcam C270)

[Device Information]
| Device Manufacturer: | N/A
| Product Name: | N/A
| Serial Number: | CC435D20
| USB Version Supported: | 2.00
| USB Device Speed: | USB 2.0 High-speed
| Driver Description: | Logitech USB Camera (HD Webcam C270)
| Hardware ID: | USB\VID_046D&PID_0825
[Driver Information]
| Driver Manufacturer: | Logitech
| Driver Description: | Logitech USB Camera (HD Webcam C270)
| Driver Provider: | Logitech
| Driver Version: | 13.51.823.0
| Driver Date: | 21-Sep-2012
| DeviceInstanceId | USB\VID_046D&PID_0825\CC435D20
| Location Paths | PCIROOT(0)#PCI(0201)#USBROOT(0)#USB(1)

[Port2] : No Device Connected

[Port3] : No Device Connected

[Port4] : No Device Connected

[Port5] : No Device Connected

[Port6] : No Device Connected

[Port7] : No Device Connected

[Port8] : No Device Connected

[Port9] : Запоминающее устройство для USB

[Device Information]
| Device Manufacturer: | Generic
| Product Name: | Mass Storage Device
| Serial Number: | 058F312D81B
| USB Version Supported: | 2.00
| USB Device Speed: | USB 2.0 High-speed
| Driver Description: | Запоминающее устройство для USB
| Hardware ID: | USB\VID_058F&PID_6362
[Driver Information]
| Driver Manufacturer: | USB-совместимое запоминающее устройство
| Driver Description: | Запоминающее устройство для USB
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.19144
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | USB\VID_058F&PID_6362\058F312D81B
| Location Paths | PCIROOT(0)#PCI(0201)#USBROOT(0)#USB(9)

[Port10] : No Device Connected

NVIDIA MCP61 - PCI-to-PCI Bridge

[General Information]
| Device Name: | NVIDIA MCP61 - PCI-to-PCI Bridge
| Original Device Name: | NVIDIA MCP61 - PCI-to-PCI Bridge
| Device Class: | PCI-to-PCI Bridge
| Revision ID: | A1
| PCI Address (Bus:Device:Function) Number: | 0:4:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03F3&SUBSYS_00000000&REV_A1
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - PCI
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03F3&SUBSYS_83A41043&REV_A1\3&267A616A&0&20
| Location Paths | PCIROOT(0)#PCI(0400)

PCI Bus #1

NVIDIA MCP61 - High Definition Audio Controller

[General Information]
| Device Name: | NVIDIA MCP61 - High Definition Audio Controller
| Original Device Name: | NVIDIA MCP61 - High Definition Audio Controller
| Device Class: | Mixed mode device
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:5:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03F0&SUBSYS_837F1043&REV_A2
[System Resources]
| Interrupt Line: | IRQ20
| Interrupt Pin: | INTB#
| Memory Base Address 0 | DFEF8000
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | Microsoft
| Driver Description: | Контроллер High Definition Audio (Microsoft)
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 19-Nov-2010
| DeviceInstanceId | PCI\VEN_10DE&DEV_03F0&SUBSYS_837F1043&REV_A2\3&267A616A&0&28
| Location Paths | PCIROOT(0)#PCI(0500)

NVIDIA MCP61 - Parallel ATA Controller

[General Information]
| Device Name: | NVIDIA MCP61 - Parallel ATA Controller
| Original Device Name: | NVIDIA MCP61 - Parallel ATA Controller
| Device Class: | IDE Controller
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:6:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03EC&SUBSYS_83A41043&REV_A2
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
| I/O Base Address 4 | FFA0
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные IDE ATA/ATAPI контроллеры)
| Driver Description: | Стандартный двухканальный контроллер PCI IDE
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03EC&SUBSYS_83A41043&REV_A2\3&267A616A&0&30
| Location Paths | PCIROOT(0)#PCI(0600)

NVIDIA MCP61 - Network Bus Enumerator

[General Information]
| Device Name: | NVIDIA MCP61 - Network Bus Enumerator
| Original Device Name: | NVIDIA MCP61 - Network Bus Enumerator
| Device Class: | Unknown Bridge
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:7:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03EF&SUBSYS_83A41043&REV_A2
[System Resources]
| Interrupt Line: | IRQ23
| Interrupt Pin: | INTA#
| Memory Base Address 0 | DFEFD000
| I/O Base Address 1 | 0
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | NVIDIA
| Driver Description: | Сетевой контроллер NVIDIA nForce
| Driver Provider: | Microsoft
| Driver Version: | 1.0.1.211
| Driver Date: | 17-Oct-2008
| DeviceInstanceId | PCI\VEN_10DE&DEV_03EF&SUBSYS_83A41043&REV_A2\3&267A616A&0&38
| Location Paths | PCIROOT(0)#PCI(0700)

NVIDIA MCP61 - SATA Controller

[General Information]
| Device Name: | NVIDIA MCP61 - SATA Controller
| Original Device Name: | NVIDIA MCP61 - SATA Controller
| Device Class: | IDE Controller
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:8:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03F6&SUBSYS_83A41043&REV_A2
[System Resources]
| Interrupt Line: | IRQ20
| Interrupt Pin: | INTA#
| I/O Base Address 0 | D400
| I/O Base Address 1 | D080
| I/O Base Address 2 | D000
| I/O Base Address 3 | CC00
| I/O Base Address 4 | C880
| Memory Base Address 5 | DFEFC000
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Capable
| Fast Back-to-Back Transactions: | Capable
[Driver Information]
| Driver Manufacturer: | NVIDIA Corporation
| Driver Description: | Контроллер NVIDIA nForce Serial ATA
| Driver Provider: | NVIDIA Corporation
| Driver Version: | 10.6.0.19
| Driver Date: | 06-Aug-2010
| DeviceInstanceId | PCI\VEN_10DE&DEV_03F6&SUBSYS_83A41043&REV_A2\3&267A616A&0&40
| Location Paths | PCIROOT(0)#PCI(0800)

NVIDIA MCP61 - PCI Express Root Port

[General Information]
| Device Name: | NVIDIA MCP61 - PCI Express Root Port
| Original Device Name: | NVIDIA MCP61 - PCI Express Root Port
| Device Class: | PCI-to-PCI Bridge
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:9:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03E8&SUBSYS_00000000&REV_A2
[PCI Express]
| Version: | 1.1
| Maximum Link Width: | 16x
| Current Link Width: | 16x
| Maximum Link Speed: | 2.5 GT/s
| Current Link Speed: | 2.5 GT/s
| Device/Port Type: | Root Port of PCI Express Root Complex
| Slot Implemented: | Yes
| Hot-Plug: | Not Capable
| Hot-Plug Surprise: | Not Capable
| Slot Power Limit: | 75.000 W
| Emergency Power Reduction: | Not Supported
| Active State Power Management (ASPM) Support: | L0s and L1
| Active State Power Management (ASPM) Status: | Disabled
| L0s Exit Latency: | 256 - 512 ns
| L1 Exit Latency: | 2 - 4 us
| Maximum Payload Size Supported: | 256 bytes
| Maximum Payload Size: | 128 bytes
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - PCI
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03E8&SUBSYS_000010DE&REV_A2\3&267A616A&0&48
| Location Paths | PCIROOT(0)#PCI(0900)

PCI Express x16 Bus #2

ATI Radeon HD 5770 1GB GDDR5

[General Information]
| Device Name: | ATI Radeon HD 5770 1GB GDDR5
| Original Device Name: | ATI/AMD Radeon HD 5770 (JUNIPER XT)
| Device Class: | VGA Compatible Adapter
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 2:0:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1002&DEV_68B8&SUBSYS_25431002&REV_00
[PCI Express]
| Version: | 1.1
| Maximum Link Width: | 16x
| Current Link Width: | 16x
| Maximum Link Speed: | 2.5 GT/s
| Current Link Speed: | 2.5 GT/s
| Device/Port Type: | Legacy PCI Express Endpoint
| Slot Implemented: | No
| Emergency Power Reduction: | Not Supported
| Active State Power Management (ASPM) Support: | L0s and L1
| Active State Power Management (ASPM) Status: | Disabled
| L0s Exit Latency: | < 64 ns
| L1 Exit Latency: | < 1 us
| Maximum Payload Size Supported: | 256 bytes
| Maximum Payload Size: | 128 bytes
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | INTA#
| Memory Base Address 0 | C0000000
| Memory Base Address 2 | DFFE0000
| I/O Base Address 4 | E800
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | Advanced Micro Devices, Inc.
| Driver Description: | AMD Radeon HD 5700 Series
| Driver Provider: | Advanced Micro Devices, Inc.
| Driver Version: | 15.200.1062.1004 (Catalyst 15.7.1)
| Driver Date: | 03-Aug-2015
| DeviceInstanceId | PCI\VEN_1002&DEV_68B8&SUBSYS_25431002&REV_00\4&210A641E&0&0048
| Location Paths | PCIROOT(0)#PCI(0900)#PCI(0000)

ATI/AMD Juniper/Broadway/Granville - High Definition Audio Controller

[General Information]
| Device Name: | ATI/AMD Juniper/Broadway/Granville - High Definition Audio Controller
| Original Device Name: | ATI/AMD Juniper/Broadway/Granville - High Definition Audio Controller
| Device Class: | Mixed mode device
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 2:0:1
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1002&DEV_AA58&SUBSYS_AA581002&REV_00
[PCI Express]
| Version: | 1.1
| Maximum Link Width: | 16x
| Current Link Width: | 16x
| Maximum Link Speed: | 2.5 GT/s
| Current Link Speed: | 2.5 GT/s
| Device/Port Type: | Legacy PCI Express Endpoint
| Slot Implemented: | No
| Emergency Power Reduction: | Not Supported
| Active State Power Management (ASPM) Support: | L0s and L1
| Active State Power Management (ASPM) Status: | Disabled
| L0s Exit Latency: | < 64 ns
| L1 Exit Latency: | < 1 us
| Maximum Payload Size Supported: | 256 bytes
| Maximum Payload Size: | 128 bytes
[System Resources]
| Interrupt Line: | IRQ17
| Interrupt Pin: | INTB#
| Memory Base Address 0 | DFFBC000
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | Microsoft
| Driver Description: | Контроллер High Definition Audio (Microsoft)
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 19-Nov-2010
| DeviceInstanceId | PCI\VEN_1002&DEV_AA58&SUBSYS_AA581002&REV_00\4&210A641E&0&0148
| Location Paths | PCIROOT(0)#PCI(0900)#PCI(0001)

NVIDIA MCP61 - PCI Express Root Port

[General Information]
| Device Name: | NVIDIA MCP61 - PCI Express Root Port
| Original Device Name: | NVIDIA MCP61 - PCI Express Root Port
| Device Class: | PCI-to-PCI Bridge
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:11:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03E9&SUBSYS_00000000&REV_A2
[PCI Express]
| Version: | 1.1
| Maximum Link Width: | 1x
| Current Link Width: | 1x
| Maximum Link Speed: | 2.5 GT/s
| Current Link Speed: | 2.5 GT/s
| Device/Port Type: | Root Port of PCI Express Root Complex
| Slot Implemented: | Yes
| Hot-Plug: | Not Capable
| Hot-Plug Surprise: | Not Capable
| Slot Power Limit: | 10.000 W
| Emergency Power Reduction: | Not Supported
| Active State Power Management (ASPM) Support: | L0s and L1
| Active State Power Management (ASPM) Status: | Disabled
| L0s Exit Latency: | 256 - 512 ns
| L1 Exit Latency: | 2 - 4 us
| Maximum Payload Size Supported: | 256 bytes
| Maximum Payload Size: | 128 bytes
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - PCI
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03E9&SUBSYS_000010DE&REV_A2\3&267A616A&0&58
| Location Paths | PCIROOT(0)#PCI(0B00)

PCI Express x1 Bus #3

NVIDIA MCP61 - PCI Express Root Port

[General Information]
| Device Name: | NVIDIA MCP61 - PCI Express Root Port
| Original Device Name: | NVIDIA MCP61 - PCI Express Root Port
| Device Class: | PCI-to-PCI Bridge
| Revision ID: | A2
| PCI Address (Bus:Device:Function) Number: | 0:12:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_10DE&DEV_03E9&SUBSYS_00000000&REV_A2
[PCI Express]
| Version: | 1.1
| Maximum Link Width: | 1x
| Current Link Width: | 1x
| Maximum Link Speed: | 2.5 GT/s
| Current Link Speed: | 2.5 GT/s
| Device/Port Type: | Root Port of PCI Express Root Complex
| Slot Implemented: | Yes
| Hot-Plug: | Not Capable
| Hot-Plug Surprise: | Not Capable
| Slot Power Limit: | 10.000 W
| Emergency Power Reduction: | Not Supported
| Active State Power Management (ASPM) Support: | L0s and L1
| Active State Power Management (ASPM) Status: | Disabled
| L0s Exit Latency: | 256 - 512 ns
| L1 Exit Latency: | 2 - 4 us
| Maximum Payload Size Supported: | 256 bytes
| Maximum Payload Size: | 128 bytes
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Enabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - PCI
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_10DE&DEV_03E9&SUBSYS_000010DE&REV_A2\3&267A616A&0&60
| Location Paths | PCIROOT(0)#PCI(0C00)

PCI Express x1 Bus #4

AMD Family 10h CPU - HyperTransport Technology Configuration

[General Information]
| Device Name: | AMD Family 10h CPU - HyperTransport Technology Configuration
| Original Device Name: | AMD Family 10h CPU - HyperTransport Technology Configuration
| Device Class: | Host-to-PCI Bridge
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 0:24:0
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1022&DEV_1200&SUBSYS_00000000&REV_00
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - CPU
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_1022&DEV_1200&SUBSYS_00000000&REV_00\3&267A616A&0&C0
| Location Paths | PCIROOT(0)#PCI(1800)

AMD Family 10h CPU - Address Map

[General Information]
| Device Name: | AMD Family 10h CPU - Address Map
| Original Device Name: | AMD Family 10h CPU - Address Map
| Device Class: | Host-to-PCI Bridge
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 0:24:1
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1022&DEV_1201&SUBSYS_00000000&REV_00
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - CPU
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_1022&DEV_1201&SUBSYS_00000000&REV_00\3&267A616A&0&C1
| Location Paths | PCIROOT(0)#PCI(1801)

AMD Family 10h CPU - DRAM Controller

[General Information]
| Device Name: | AMD Family 10h CPU - DRAM Controller
| Original Device Name: | AMD Family 10h CPU - DRAM Controller
| Device Class: | Host-to-PCI Bridge
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 0:24:2
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1022&DEV_1202&SUBSYS_00000000&REV_00
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - CPU
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_1022&DEV_1202&SUBSYS_00000000&REV_00\3&267A616A&0&C2
| Location Paths | PCIROOT(0)#PCI(1802)

AMD Family 10h CPU - Miscellaneous Control

[General Information]
| Device Name: | AMD Family 10h CPU - Miscellaneous Control
| Original Device Name: | AMD Family 10h CPU - Miscellaneous Control
| Device Class: | Host-to-PCI Bridge
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 0:24:3
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1022&DEV_1203&SUBSYS_00000000&REV_00
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - CPU
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_1022&DEV_1203&SUBSYS_00000000&REV_00\3&267A616A&0&C3
| Location Paths | PCIROOT(0)#PCI(1803)
[Northbridge Capabilities]
| Internal Node Number: | Node0
| Multi-Node Capability: | Not Capable
| L3 Cache: | Present
| Link3 Unganging: | Not Enabled
| Link2 Unganging: | Not Enabled
| Link1 Unganging: | Not Enabled
| Link0 Unganging: | Not Enabled
| Multi-Processor Capability: | 1 CPU
| Multiple VID Plane Capability: | Not Capable
| Multi-Core Capability: | Quad-Core
| Link Error-Retry: | Capable
| Hardware Thermal Control (HTC): | Capable
| SVM: | Capable
| On-chip Memory Controller: | Present
| Maximum DRAM Frequency: | 667 MHz
| Chip-Kill ECC: | Capable
| ECC: | Capable
| Eight-Node Multi-Processor (Big-MP): | Not Capable
| Dual-Node Multi-Processor (MP): | Not Capable
| Dual-Channel (128-Bit) DRAM: | Capable

AMD Family 10h CPU - Link Control

[General Information]
| Device Name: | AMD Family 10h CPU - Link Control
| Original Device Name: | AMD Family 10h CPU - Link Control
| Device Class: | Host-to-PCI Bridge
| Revision ID: | 0
| PCI Address (Bus:Device:Function) Number: | 0:24:4
| PCI Latency Timer: | 0
| Hardware ID: | PCI\VEN_1022&DEV_1204&SUBSYS_00000000&REV_00
[System Resources]
| Interrupt Line: | N/A
| Interrupt Pin: | N/A
[Features]
| Bus Mastering: | Disabled
| Running At 66 MHz: | Not Capable
| Fast Back-to-Back Transactions: | Not Capable
[Driver Information]
| Driver Manufacturer: | (Стандартные системные устройства)
| Driver Description: | Стандартный мост PCI - CPU
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.17514
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | PCI\VEN_1022&DEV_1204&SUBSYS_00000000&REV_00\3&267A616A&0&C4
| Location Paths | PCIROOT(0)#PCI(1804)

Video Adapter

AMD Radeon HD 5770

[Video chipset]
| Video Chipset: | AMD Radeon HD 5770
| Video Chipset Codename: | JUNIPER XT
| Video Memory: | 1024 MBytes of GDDR5 SDRAM [Samsung]
[Video Card]
| Video Card: | ATI Radeon HD 5770 1GB GDDR5
| Video Bus: | PCIe v1.1 x16 (2.5 GT/s) @ x16 (2.5 GT/s)
| Video RAMDAC: | Internal DAC(400MHz)
| Video BIOS Version: | 012.013.000.001.034705
[Performance]
| Processor Clock: | 157.0 MHz
| Memory Clock: | 300.0 MHz (Effective 1200.0 MHz)
| Memory Bus Width: | 128-bit
| Number Of ROPs: | 16
| Number Of Unified Shaders: | 800
| Number Of TMUs (Texture Mapping Units): | 40
| ASIC Quality: | 44.4 %
| Hardware ID: | PCI\VEN_1002&DEV_68B8&SUBSYS_25431002&REV_00
| PCI Location (Bus:Dev:Fnc): | 2:00:0
[Driver Information]
| Driver Manufacturer: | Advanced Micro Devices, Inc.
| Driver Description: | AMD Radeon HD 5700 Series
| Driver Provider: | Advanced Micro Devices, Inc.
| Driver Version: | 15.200.1062.1004 (Catalyst 15.7.1)
| Driver Date: | 03-Aug-2015
| DeviceInstanceId | PCI\VEN_1002&DEV_68B8&SUBSYS_25431002&REV_00\4&210A641E&0&0048
| Location Paths | PCIROOT(0)#PCI(0900)#PCI(0000)

Monitor

BenQ GL2450H (Digital)

[General information]
| Monitor Name: | BenQ GL2450H (Digital)
| Monitor Name (Manuf): | BenQ GL2450H
| Serial Number: | 87D04388019
| Date Of Manufacture: | Week: 28, Year: 2013
| Monitor Hardware ID: | Monitor\BNQ78A7
| Max. Vertical Size: | 30 cm
| Max. Horizontal Size: | 53 cm
| Horizontal Frequency: | 30 - 83 kHz
| Vertical Frequency: | 50 - 76 Hz
| Maximum Pixel Clock: | 170 MHz
[Advanced parameters]
| Input Signal: | Digital
| Display Type: | RGB color
| Gamma Factor: | 2.20
[DPMS Modes]
| Standby: | Not Supported
| Suspend: | Not Supported
| Active Off: | Supported
| Standard Colour Space: | Supported
| Preferred Timing Mode: | Supported
| Default GTF Supported: | Not Supported
| DFP 1.x Compatible: | No
[Supported Video Modes]
| 1280 x 800 | 60 Hz
| 1280 x 720 | 60 Hz
| 1280 x 1024 | 60 Hz
| 1600 x 900 | 60 Hz
| 1680 x 1050 | 60 Hz
| 1920 x 1080 | 60 Hz
| 1920 x 1080 | 531 x 298 mm, Pixel Clock 148.50 MHz

Drives

(S)ATA/ATAPI Drives

ADATA SP550

[General Information]
| Drive Controller: | Serial ATA 6Gb/s @ 3Gb/s
| Drive Model: | ADATA SP550
| Drive Revision: | P0705AB
| Drive Serial Number: | 2G3920053564
| Drive Capacity: | 228,936 MBytes (240 GB)
| Drive Capacity [MB]: | 228936
| Media Rotation Rate: | SSD Drive (Non-rotating)
| ATA Major Version Supported: | ATA/ATAPI-5, ATA/ATAPI-6, ATA/ATAPI-7, ATA8-ACS, ACS-2
| ATA Transport Version Supported: | SATA 3.1
[Drive Geometry]
| Number of Cylinders: | 16383
| Number of Heads: | 16
| Sectors Per Track: | 63
| Number of Sectors: | 16514064
| Total 32-bit LBA Sectors: | 268435455
| Total 48-bit LBA Sectors: | 468862128
| Logical Sector Size: | 512 Bytes
| Cache Buffer Size: | N/A
[Transfer Modes]
| Sectors Per Interrupt: | Total: 2, Active: 2
| Max. PIO Transfer Mode: | 4
| Multiword DMA Mode: | Total: 2, Active: -
| Singleword DMA Mode: | Total: -, Active: -
| Ultra-DMA Mode: | Total: 6 (ATA-133), Active: 6 (ATA-133)
| Max. Multiword DMA Transfer Rate: | 16.7 MBytes/s
| Max. PIO with IORDY Transfer Rate: | 16.7 MBytes/s
| Max. PIO w/o IORDY Transfer Rate: | 16.7 MBytes/s
| Native Command Queuing: | Supported, Max. Depth: 32
| TRIM Command: | Supported (Deterministic Read After TRIM, Words = 0)
[Device flags]
| Fixed Drive: | Present
| Removable Drive: | Not Present
| Magnetic Storage: | Present
| LBA Mode: | Supported
| DMA Mode: | Supported
| IORDY: | Supported
| IORDY Disableable: | Supported
[Features]
| Write Cache: | Present, Active
| S.M.A.R.T. Feature: | Present, Active
| Security Feature: | Present, Inactive
| Removable Media Feature: | Not Present, Disabled
| Power Management: | Present, Active
| Advanced Power Management: | Not Present, Inactive
| Packet Interface: | Not Present, Disabled
| Look-Ahead Buffer: | Present, Active
| Host Protected Area: | Present, Enabled
| Power-Up In Standby: | Not Suppported, Inactive
| Automatic Acoustic Management: | Not Suppported, Inactive
| 48-bit LBA: | Supported, Active
| Host-Initiated Link Power Management: | Supported
| Device-Initiated Link Power Management: | Supported, Disabled
| In-Order Data Delivery: | Not Supported
| Hardware Feature Control: | Not Supported
| Software Settings Preservation: | Supported, Enabled
| NCQ Autosense: | Not Supported
| Link Power State Device Sleep: | Supported, Disabled
| Hybrid Information Feature: | Not Supported
| Rebuild Assist: | Not Supported
| Power Disable: | Not Supported
| All Write Cache Non-Volatile: | Not Supported
| Extended Number of User Addressable Sectors: | Not Supported
| CFast Specification: | Not Supported
| NCQ Priority Information: | Not Supported
| Host Automatic Partial to Slumber Transitions: | Not Supported
| Device Automatic Partial to Slumber Transitions: | Not Supported
| NCQ Streaming: | Not Supported
| NCQ Queue Management Command: | Not Supported
| DevSleep to Reduced Power State: | Supported
| Extended Power Conditions Feature: | Not Supported
| Sense Data Reporting Feature: | Not Supported
| Free-Fall Control Feature: | Not Supported
| Write-Read-Verify Feature: | Not Supported
[Security]
| Security Feature: | Supported
| Security Status: | Disabled
| Security Locked: | Disabled
| Security Frozen: | Enabled
| Enhanced Security Erase: | Supported
| Sanitize Feature: | Supported
| Sanitize Device - Crypto Scramble: | Not Supported
| Sanitize Device - Overwrite: | Not Supported
| Sanitize Device - Block Erase: | Supported
| Sanitize Device - Antifreeze Lock: | Not Supported
| Device Encrypts All User Data: | Not Supported
| Trusted Computing: | Not Supported
[Self-Monitoring, Analysis and Reporting Technology (S.M.A.R.T.)]
| [01] Raw Read Error Rate: | 100/Always OK, Worst: 100
| [05] Reallocated Sector Count: | 100/Always OK, Worst: 100
| [09] Power-On Hours/Cycle Count: | 100/Always OK, Worst: 100 (657 hours / 27.4 days)
| [0C] Power Cycle Count: | 100/Always OK, Worst: 100 (Data = 633,0)
| [A0] Uncorrectable Sector Count: | 100/Always OK, Worst: 100
| [A1] Valid Spare Blocks: | 100/Always OK, Worst: 100 (Data = 32,0)
| [A3] Unknown | 100/Always OK, Worst: 100 (Data = 259,0)
| [94] Unknown | 100/Always OK, Worst: 100 (Data = 119491,0)
| [95] Unknown | 100/Always OK, Worst: 100 (Data = 1635,0)
| [96] Unknown | 100/Always OK, Worst: 100 (Data = 1463,0)
| [97] Unknown | 100/Always OK, Worst: 100 (Data = 1614,0)
| [A4] Unknown | 100/Always OK, Worst: 100 (Data = 98396,0)
| [A5] Maximum TLC Erase Count: | 100/Always OK, Worst: 100 (Data = 125,0)
| [A6] Minimum TLC Erase Count: | 100/Always OK, Worst: 100 (Data = 24,0)
| [A7] Average TLC Erase Count: | 100/Always OK, Worst: 100 (Data = 76,0)
| [A9] Percentage Lifetime Remaining: | 100/1, Worst: 100 (Data = 94,0)
| [B5] Program Fail Count (Total): | 100/Always OK, Worst: 100
| [B6] Erase Fail Count (Total): | 100/Always OK, Worst: 100
| [C0] Power-off Retract Count: | 100/Always OK, Worst: 100 (Data = 48,0)
| [C2] Temperature | 100/70, Worst: 100 (23.0 °C)
| [C7] SATA CRC Error Count: | 100/Always OK, Worst: 100
| [E8] Available Reserved Space: | 100/Always OK, Worst: 100 (Data = 100,0)
| [F1] Total Host Writes: | 100/Always OK, Worst: 100 (Data = 170319,0)
| [F2] Total Host Reads: | 100/Always OK, Worst: 100 (Data = 271843,0)
| [F5] Total TLC Write Count: | 100/Always OK, Worst: 100 (Data = 581151,0)
| [F6] Total SLC Write Count: | 100/Always OK, Worst: 100 (Data = 238982,0)
| [F7] RAID Recovery Count: | 100/Always OK, Worst: 100
| Drive Remaining Life | 100%

WDC WD50 00AAKS-00V1A

[General information]
| Drive Model: | WDC WD50 00AAKS-00V1A
| Drive Revision: | 05.0
| Device Type: | Disk drive

Audio

NVIDIA MCP61 - High Definition Audio Controller

| Audio Adapter: | NVIDIA MCP61 - High Definition Audio Controller
| Audio Controller Hardware ID: | PCI\VEN_10DE&DEV_03F0&SUBSYS_837F1043&REV_A2
| High Definition Audio Codec: | RealTek ALC662
| Audio Codec Hardware ID: | HDAUDIO\FUNC_01&VEN_10EC&DEV_0662&SUBSYS_00000000
[Driver Information]
| Driver Manufacturer: | Realtek
| Driver Description: | Realtek High Definition Audio
| Driver Provider: | Realtek Semiconductor Corp.
| Driver Version: | 6.0.1.8004
| Driver Date: | 29-Nov-2016
| DeviceInstanceId | HDAUDIO\FUNC_01&VEN_10EC&DEV_0662&SUBSYS_1043837F&REV_1001\4&26DF25D7&0&0001

ATI/AMD Juniper/Broadway/Granville - High Definition Audio Controller

| Audio Adapter: | ATI/AMD Juniper/Broadway/Granville - High Definition Audio Controller
| Audio Controller Hardware ID: | PCI\VEN_1002&DEV_AA58&SUBSYS_AA581002&REV_00
| High Definition Audio Codec: | ATi RADEON HDMI
| Audio Codec Hardware ID: | HDAUDIO\FUNC_01&VEN_1002&DEV_AA01&SUBSYS_00000000
[Driver Information]
| Driver Manufacturer: | Advanced Micro Devices
| Driver Description: | AMD High Definition Audio Device
| Driver Provider: | Advanced Micro Devices
| Driver Version: | 7.12.0.7722
| Driver Date: | 04-Jun-2015
| DeviceInstanceId | HDAUDIO\FUNC_01&VEN_1002&DEV_AA01&SUBSYS_00AA0100&REV_1002\5&2ECDDAB2&0&0001

Network

Адаптер D-Link DFE-520TX PCI Fast Ethernet

[General information]
| Network Card: | Адаптер D-Link DFE-520TX PCI Fast Ethernet
| Vendor Description: | Unknown
| MAC Address: | Unknown
[Capabilities]
| Maximum Link Speed: | Unknown
| Transmit Buffer Size: | Unknown
| Receive Buffer Size: | Unknown

Сетевой контроллер NVIDIA nForce

[General information]
| Network Card: | Сетевой контроллер NVIDIA nForce
| Vendor Description: | NVIDIA nForce MCP Networking Adapter Driver
| MAC Address: | 00-26-18-E6-E7-AF
[Capabilities]
| Maximum Link Speed: | 100 Mbps
| Transmit Buffer Size: | 3100672 Bytes
| Receive Buffer Size: | 6201344 Bytes

Ports

Serial Ports

Parallel Ports

USB

Стандартный OpenHCD USB хост-контроллер

Root Hub

[Port1] : No Device Connected

[Port2] : No Device Connected

[Port3] : Составное USB устройство

[Device Information]
| Device Manufacturer: | A4TECH
| Product Name: | USB Device
| Serial Number: | N/A
| USB Version Supported: | 1.10
| USB Device Speed: | USB 1.1 Full-speed
| Driver Description: | Составное USB устройство
| Hardware ID: | USB\VID_09DA&PID_9090
[Driver Information]
| Driver Manufacturer: | (Стандартный USB хост-контроллер)
| Driver Description: | Составное USB устройство
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.23933
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | USB\VID_09DA&PID_9090\5&13FF92DD&0&3
| Location Paths | PCIROOT(0)#PCI(0200)#USBROOT(0)#USB(3)

[Port4] : No Device Connected

[Port5] : No Device Connected

[Port6] : No Device Connected

[Port7] : No Device Connected

[Port8] : No Device Connected

[Port9] : No Device Connected

[Port10] : No Device Connected

Стандартный расширенный PCI - USB хост-контроллер

Root Hub

[Port1] : Logitech USB Camera (HD Webcam C270)

[Device Information]
| Device Manufacturer: | N/A
| Product Name: | N/A
| Serial Number: | CC435D20
| USB Version Supported: | 2.00
| USB Device Speed: | USB 2.0 High-speed
| Driver Description: | Logitech USB Camera (HD Webcam C270)
| Hardware ID: | USB\VID_046D&PID_0825
[Driver Information]
| Driver Manufacturer: | Logitech
| Driver Description: | Logitech USB Camera (HD Webcam C270)
| Driver Provider: | Logitech
| Driver Version: | 13.51.823.0
| Driver Date: | 21-Sep-2012
| DeviceInstanceId | USB\VID_046D&PID_0825\CC435D20
| Location Paths | PCIROOT(0)#PCI(0201)#USBROOT(0)#USB(1)

[Port2] : No Device Connected

[Port3] : No Device Connected

[Port4] : No Device Connected

[Port5] : No Device Connected

[Port6] : No Device Connected

[Port7] : No Device Connected

[Port8] : No Device Connected

[Port9] : Запоминающее устройство для USB

[Device Information]
| Device Manufacturer: | Generic
| Product Name: | Mass Storage Device
| Serial Number: | 058F312D81B
| USB Version Supported: | 2.00
| USB Device Speed: | USB 2.0 High-speed
| Driver Description: | Запоминающее устройство для USB
| Hardware ID: | USB\VID_058F&PID_6362
[Driver Information]
| Driver Manufacturer: | USB-совместимое запоминающее устройство
| Driver Description: | Запоминающее устройство для USB
| Driver Provider: | Microsoft
| Driver Version: | 6.1.7601.19144
| Driver Date: | 21-Jun-2006
| DeviceInstanceId | USB\VID_058F&PID_6362\058F312D81B
| Location Paths | PCIROOT(0)#PCI(0201)#USBROOT(0)#USB(9)

[Port10] : No Device Connected